|  |  |  |  |
| --- | --- | --- | --- |
| **REV REQ NO.** | **DESCRIPTION** | **URGENT** | **ERCOT Opinion** |
| **953NPRR** | **Addition of Relay Loadability Rating Definition.** This Nodal Protocol Revision Request (NPRR) adds the Relay Loadability Rating definition in order to address the North American Electric Reliability Corporation (NERC) definition changes for Operational Planning Analysis and Real Time Assessments which adds a requirement to include protection system limitations. These changes also support ERCOT housing and monitoring the Relay Loadability Rating in Energy Management System (EMS) applications. [ERCOT] | N | ERCOT supports approval of NPRR953 |
| **997NPRR** | **Natural Gas Pipeline Coordination Requirements for Resource Entities with Natural Gas Generation Resources.** This NPRR requires a Resource Entity that controls a Generation Resource that relies on natural gas as its primary fuel source to submit a declaration contained in the summer weather preparedness form to ERCOT stating that the Resource Entity or the Resource Entity’s Qualified Scheduling Entity (QSE) has made a written effort to communicate with the operator of each natural gas pipeline that is directly connected to the Resource Entity’s Generation Resource to coordinate any planned pipeline outages to maximize the Generation Resource’s availability during the summer Peak Load Season of that year. [ERCOT] | Y | ERCOT supports approval of NPRR997 |
| **998NPRR** | **ERS Deployment and Recall Messages.** This Nodal Protocol Revision Request (NPRR) establishes a requirement for ERCOT to post a message to the Market Information System (MIS) Public Area every time ERS is deployed or recalled. [ERCOT] | Y | ERCOT supports approval of NPRR998 |
| **075PGRR** | **Dynamic Model Quality Requirement.** This Planning Guide Revision Request (PGRR) adds a requirement for Resource Entities and Interconnecting Entities (IEs) to provide model quality test results that demonstrate appropriate performance for submitted dynamic models. [ERCOT] | N | ERCOT supports approval of PGRR075 |