**Section 2:**

NPRR1145 – Use of State Estimator-Calculated ERCOT-Wide TLFs in Lieu of Seasonal Base Case ERCOT-Wide TLFs for Settlement

This Nodal Protocol Revision Request (NPRR) changes the 15-minute level ERCOT-wide Transmission Loss Factors (TLFs) that are used in the Settlement process from seasonal base case TLFs to State Estimator-calculated TLFs in the Energy Management System (EMS). It also clarifies the use of Non-Opt-In Entity (NOIE) deemed actual TLFs to remove behind-the-meter Transmission Losses.

Revised Subsection: 2.1 [unboxed due to system implementation]

**Section 13:**

NPRR1145 – Use of State Estimator-Calculated ERCOT-Wide TLFs in Lieu of Seasonal Base Case ERCOT-Wide TLFs for Settlement

*See Section 2 above.*

Revised Subsections: 13.1.1, 13.1.2, 13.2.2, 13.2.3, 13.2.4, 13.2.5, 13.2.5 (new), 13.4, and 13.4.1 [unboxed due to system implementation]